Installation steps:

STEP 1) Unzip G2SOFT.ZIP to destination directory (e.g. C:\Program Files\G2SOFT)
STEP 2) Connect GSC-2/GSC-3 to PC using USB A-B cable.
	Install appropriate USB drivers:
             - for Windows XP or Vista from "Windows XP_VISTA\USB_DRIVERS" directory,
             - for Windows 98 or ME from "Windows 98_ME\USB_DRIVERS" directory,

STEP 3) Run G2SOFT.EXE from appropriate directory. In Windows XP/Vista G2SOFT automatically 
        detects connected GSC-2/GSC-3; in Windows 98/ME you must enter virtual serial port number.


In case you do not have GSC-2/GSC-3 you can also use G2SOFT in standalone (offline) mode.


	
	
